PKU1200M new from HMI Systems

Learn more at [www.hmisystems.net](http://www.hmisystems.net/)



Standard Product Features

* **256 step brightness control for each color**
* **New LED visual effects (blink, pulse, spin, ripple, split)**
* **On/Off, momentary, toggle, scroll/step functions programmable for each key**
* **Autonomous operation (key press causes LED to change state without feedback from external device)**
* **NMEA200 bus compliant (support ISO requests, address claim, binary status 127501 and binary control 127502 messages)**
* **CAN Open**
* **J1939**
* **NMEA2000**
* **Free Software Utility**
* **Accessories Catalog**
* **Connector Options include Deutsch, Molex and more**

Protocols & Accessories

with Designer Firmware Firmware

Improved Product Features

* **Supply Voltage 12-24V**
* **Brighter LED’s**
* **Relegendable Buttons**
* **Multicolor indicator rings**
* **Sealed IP68**
* **Vertical or horizontal mount**
* **CRM, Designer, ECS firmware options**
* **Improved thermal dissipation**
* **Full color LED indicators including pure white**
* **Standard and custom legends (no mins, no set up fees)**
* **All LEDs active power consumption only 70 mA @ 12V**
* **Simplified CAN messaging using CANconnect software to control multiple LEDs within single message**
* **3 extra status LEDs with independent control**



1955 West State Rd 426 | Oviedo, FL 32765 | Tel: 407.359.8171 | Fax: 407.359.8170

[info@hmisystems.net](mailto:info@hmisystems.net) | [www.hmisystems.net](http://www.hmisystems.net/)

